**Notes for EDYC RO 2021 version 5**

**Due to RRS rule change we cannot use flag V for a class flag – hence we will use flag T for the Dinghy II**

**Due to Covid – we seek flag movements to be conducted by one person – thus no hauling up and down at the same time point.**

Warning signal times

|  |  |  |
| --- | --- | --- |
| **CLASSES** | **Saturday** | **Wednesday** |
| Cruiser 1 Handicap (PYS 1045 & under) | 1420 | 1920 |
| Cruiser 2 Handicap (PYS 1046 & over) | 1423 | 1923 |
| Dinghy 1 Handicap (PYS 1140 & under) | 1426(Race 1)  No later than 1545(Race 2) | 1926 |
| Leisure 17 | 1429 | 1929 |
| Dinghy 2 Handicap (PYS 1141 & over) | 1432(Race 1)  No later than 1548(Race 2) | 1932 |

Class flags shall be the following [Code Flags](http://www.edyc.co.uk/ood-halyard-flag-diagram.htm):

|  |  |
| --- | --- |
| **Class** | **Code Flag** |
| Cruiser 1 | H |
| Cruiser 2 | G |
| Dinghy 1 | W |
| Leisure 17 | B |
| Dinghy 2 | ~~V~~ now T |

OTHER FLAGS

First Substitute, P, S – standard meanings

The RO will commence with seven flags raised on halyards and stick, flying and visible on the halyards well before 14:20, the AP flag will be used and fly on rear of committee boat on stick, no sound signals will have been made

The Autohoot will be set for 3 mn repetitive hoots

The warning signal for each succeeding class will be the starting signal of the preceding class. Except in the case of cruiser I where the warning signal is the lowering of the Blue flag. There are no preparatory signals.

At 14:17 the AP flag stick will be removed – auto hoot started

At 14:20 the Blue flag will be lowered – the warning signal for cruiser I

At 14:23 the H flag will be lowered the start signal for Cruiser I

Also this is the warning signal for Cruiser II

At 14:26 the G flag will be lowered the start signal for Cruiser II

Also this is the warning signal for Dinghy I

At 14:29 the W flag will be lowered the start signal for Dinghy I


Also this is the warning signal for Leisure 17

At 14:32 the B flag will be lowered the start signal for Leisure 17

Also this is the warning signal for Dinghy II

At 14:35 the T flag will be lowered the start signal for Dinghy II

All flags are on deck and auto hoot is turned off



Flag V means Monitor communication channel for safety instructions (see rule 37).